Blinkedings Ultimate

Maintainer

yomin

Date

25.03.2013

Status

done

Resources

https://github.com/Yomin/blinkedings_ultimate

Cost

~7 Euro

Successor of Blinkedings Starterkit. Equipped with a FT232RL chip the ATTINY2313 can be flashed via USB and bootloader - no ISP needed anymore. Also the chip registers with the USB Host Controller which unlocks up to 500mA to fully utilize the rgb led.

Setup

solder all components to PCB

solder ISP header to ISP pads

flash bootloader of your choice (eg fastboot)

remove ISP header

upload your program with bootloader client of your choice (eg fboot)

profit

Pics

Prototyp Flashing the bootloader via ISP (in this hardware revision the ISP pads were wrong connected therefore the ISP is directly soldered to the die pins) done