FTDI Breakout Board

Maintainer

yomin

Date

2013-03-23

Status

finished

Resources

https://github.com/Yomin/ftdi_breakout

Cost

~4 Euro

Makes all pins of FT232RL available. Also provides LED at CBUS2 for simple use of eg RxTx activity.

The FT232RL chip is an USB-UART chip to provide serial communication with microcontrollers and even flashing of these (bootloader required).

from abouve from below